When possible, disk images were taken of original disks using ImageDisk.  Official application disks are never bootable, as CP/M was a separate $150 purchase.  To make a disk bootable, use the backup utility within CP/M to sysgen a disk, and then use the utility to copy the application disk.

I hope you found this disk image helpful; if you have any software you can contribute, know of any programs made for the SMC-70 or SMC-70G that are not on the list, or have general information to share, please reach out! mark@mailscraps.com

https://docs.google.com/spreadsheets/d/e/2PACX-1vSDa9sUw-4o2MdkQx0INAgXFGQpMDld7SgPfCcwzBlnXH83VR1FddLLhubB00lTZN4wUP2T1MUnvzCQ/pubhtml